|  |
| --- |
| **ESTABLISHMENT: ADDRESS: LOCATION: DATE:** |
| **AT THE START OF INSPECTION, THE POOL/SPA WAS: OPEN / CLOSED** |
|  |
| 1. EMERGENCY 911 PHONE/CALL BOX WORKING PROPERLY YES / NO |
| 2. MAIN DRAINS CLEARLY VISIBLE: YES / NO |
| 3. SHEPHERD’S CROOK ATTACHED TO FIBERGLASS POLE YES / NO |
| 4. RING BUOY WITH SAFETY LINE ATTACHED YES / NO |
| 5. GATE(S) SELF-CLOSING, SELF-LATCHING, FENCE SECURE YES / NO / LOCKED |
| 6. SVRS/APSS TESTED, WORKING PROPERLY YES / NO / N/A |
| 7. EMERGENCY SHUTOFF SWITCH WORKING PROPERLY YES / NO / N/A |
| 8. SPA TEMPERATURE NOT MORE THAN 104OF (and sign, 1”) YES / NO / N/A |
| 9. “No Diving” + Symbol (4”), “No Lifeguard” (4”), “Persons under 14” (2”), “Emergency, Dial 911” (4”), “No Glass” (2”), |
| Max User Load (2”), “Changing Diapers” (2”), “Ill with Diarrhea” (2”), “Breath Holding” (2”), “Pets Prohibited (2”), |
| Directions to 911 phone (2”), Location over 911 phone (1”), Hours Operation (1”), Emergency Spa Shutoff (2”) |
| REQUIRED SIGNS POSTED INSIDE POOL YARD YES / NO |
| 10.POOL / SPA CHEMISTRY CHECKED YES / NO |
| FREE CHLORINE/BROMINE: (2\*- 8 ppm Cl / 3-10 ppm pool Br, 4-10 ppm spa Br) |
| pH: (7.0 – 7.8) |
| CYANURIC ACID: (<100 ppm pool, 0 ppm spa) |
| 11.IN ADDITION: |
|  |
|  |
|  |
| **AT THE CLOSE OF INSPECTION, THE POOL/SPA IS: OPEN / CLOSED** |
| REASON(S) FOR CLOSURE: |
| **IF CLOSED, GATE(S) MUST BE LOCKED TO USERS & POOL/SPA POSTED “CLOSED.”****CONTACT ENVIRONMENTAL HEALTH FOR INSPECTION (or re-inspect) PRIOR TO OPENING**  |
| **RECEIVED BY:**(PRINT AND SIGN) DATE: |
| **INSPECTED BY**:(PRINT AND SIGN) DATE: |

**Notes:**